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FRAMEWORK INFORMATION

Following a competitive tendering process, which included submission of prices through an e-auction, the Members of Advantage South West have selected Specialist Building Contracting Ltd trading as Wrekin Windows to supply (and install if required) PVCu windows for new build (where PVCu is used), and to supply and install for planned and responsive maintenance. 
Wrekin Windows will provide the complete service directly to Advantage South West Members, including the service of acting as a Contractor/Constructor. Wrekin Windows can receive orders directly from the Advantage South West Member and can provide the complete TLO/Site control. There should normally be no need to involve a Contractor in this. 

Supplier:	Wrekin Windows, Units D1-D4, Stafford Park 4, Telford, Shropshire, TF3 3BA
Contract ref:  A1798
Contact:	Sharon Durrance					Gareth Jeffries 
Contract Controller					Regional Sales Manager 		
01952 205005					07808 364916
Sharon.Durrance@wrekin-windows.co.uk 	gjeffries@epwin.co.uk 

Overview
Retro-fit
A rolling replacement programme must be agreed with Wrekin. 
After initial contact from the Member to the tenant, Wrekin will contact the tenant to arrange the survey. This survey will be undertaken within the constraints agreed with the Member. Unless agreed otherwise with the Member, the maximum lead time from notification of requirement to survey will be 4 weeks. 
Photographs of the existing configuration and a priced schedule will be provided to the Member for agreement prior to manufacturing taking place. Maximum lead time from survey to installation unless agreed otherwise with the client is 8 weeks. The minimum lead time that Wrekin require from survey to installation is 5 weeks. 
Every surveying and installation operative entering a tenant’s home will have been CRB checked. 
New Build
The contractor must liaise with Wrekin over window sizes, program and required delivery / install dates. There is a priced option for Wrekin to install the windows.
The minimum lead time that Wrekin require from agreement of sizes to delivery is 5 weeks.  
Key product attributes
The product has the following key attributes, additional information can be found in the Specification section:
· Energy rated as “B”
· U-value max 1.4 W/m2K
· All products have Secured by Design accreditation
· FENSA registered
· 25 year design life
· Extended warranty 
· Internally beaded
· Frame mounted trickle ventilation 
· Choice of brass, white or brown handles
· Option of brown PVCu

specification
The door requirement is for a small number of French doors and sliding patio doors. It is not for front doors, back doors or utility doors for which we have a separate contract.  
Standards
1. Extrusion manufacturers to be BS 7413 and BS EN 12608:2016 accredited. 
2. Fabrication to BS7412: 2007 
3. Window Frames to be manufactured to meet the requirements of PAS 24: 2016 Enhanced security performance requirements for doorsets and windows in the UK.
4. All hardware to be manufactured to meet the requirements of PAS 24:  2016
5. BS5588:1990 Part 1 Fire precautions in the design, construction and use of buildings
6. BS6206:1981 Specification for impact performance requirements for flat safety glass and safety plastics for use in buildings (not less than Class C)
7. BS12150:2004 Glass in building. Thermally toughened soda lime silicate safety glass. Evaluation of conformity/Product standard
8. BS6262:1982 Glazing for buildings
9. BS5713:1979 Specification for hermetically sealed flat double glazing units
10. BS6375:2009 Part 1 / 2 Performance of windows and doorsets, classification for weathertightness, specification for operation and strength characteristics
11. Maintenance & cleaning - to conform with BS8213 2016 Part 1 Code - cleanable from inside the property - where practicable.
12. Installation – to conform with BS8213 2016 Part 4 Code of practice for the installation of replacement doors and windows and door sets in dwellings
13. Secured by Design accredited 
14. Doors to be kitemarked to PAS23-1 1999 and PAS24-1 2016
15. Part B Building Regs compliant (emergency egress from windows upstairs). (For avoidance of doubt all habitable first floor rooms to have egress hinges and non-locking handles)
16. Part L Building Regs compliant 
17. Part M Building Regs compliant
18. Part N Building Regs compliant
19. Window installations shall be classified as Energy Rating minimum “B” unless there is a different project-by-project requirement.
20. FENSA registered 
21. 25 year design life in accordance with BLP Construction Durability Database.
Frame
22. Manufactured from extruded hollow PVC-U to BS EN 12608 reinforced with galvanised steel, aluminium or recycled PVCu profiles to the recommendations in British Plastics Federation publication 323/1.
23. PVCu - White to BS7412.  Option for external brown colouring, retaining white internal finish (option for brown inside)
24. Profile - range from 58mm to 70mm, to relevant British Standard. Principal wall thickness c.3mm 
25. Galvanised steel/aluminium/recycled PVCu reinforced to system company recommendation
26. Standard black seal
27. All windows and doors to be fitted with adjustable trickle ventilators to meet Approved Document F of Building Regulations.
28. 28mm insulating infill panel as required
29. Windows shall be fully weather sealed. Gaskets shall be non-migratory EPDM (neoprene) or TPE to BS4255 with all seals being in one length.
30. The frames are to incorporate an adequate means of concealed self-drainage.   
31. Cill ends to be closed with plastic end caps and sealed.   
32. New build only – detachable or sliding cill to allow installation at house frame manufacturer’s premises where required.
Glass
33. All glazing to be carried out in accordance with the requirements of the Building Regulations Part N & L. Where safety glass is required on ground floor (and other floors’ vulnerable windows) it is to be laminated (except for non-vulnerable which is to be toughened); other floors’ safety glass where required is to be toughened.    
34. Glass to comply with BS 952: Part 1:1978.
35. Safety glass to comply with BS6206:1981 and BS12150:2004 regarding impact performance and the marking of glass to indicate type and classification, and with BS 6262:1982 with regard to minimum thickness for certain pane sizes. To be marked in accordance with BS6206:1981 and BS12150:2004
36. Hermetically sealed argon filled
37. Standard 28mm (4-20-4) construction 
38. Beading - 70mm Profile - internal decorative bead.  58mm/60mm profile - internal decorative/splayed bead (unless external beading is required to BS 7950, with relevant security tape) 
39. All glazing internally installed (to enable replacement of glass from within the building)
Hardware - windows
40. All hardware must be manufactured in accordance with BS EN ISO 9001:2008 Quality Assurance System and meet the requirements of BS EN 1670:2007 Class 4 for corrosion resistance.
41. Hardware with provision for adjustment shall be accessible for adjustment after the window has been installed. Hardware used to open/close the window shall be replaceable without removing the outer frame from the structure.
42. Espagnolette & rail type locking system to casements and sashes
43. Windows to be fitted with Espagnolette operating handles. Colour white. Handles to incorporate a push release mechanism with a barrel lock.  All to BS 6462-1985 strength Test C3.
44. Top hung sash - Austenitic Stainless Steel Friction Stays (>450mm Restricted, <450mm Unrestricted), require anti-jemmy device
45. Side hung sash - Austenitic Stainless Steel Friction Stays (Restricted), require anti-jemmy device
46. Offset Handle.  
47. Locking
a. Key locking standard on all vulnerable windows. 
b. Additional keys to be available at future dates.
c. 1st floor habitable room windows to be non-key locking
d. Windows required under Building Regulations to act as a fire escape route shall not have key-operated locks.  
e. Locks to be capable of securing the window in the night vent position. 
f. Each lockable window shall be supplied with a key. Each window lock in a property shall work with the same key.
48. Fixing screws are to be Austenitic stainless steel to all hardware.
49. All hinges must be manufactured in accordance with BS EN ISO 9001:2008 Quality Assurance System and meet the requirements of BS EN 1670:2007 Class 4 for corrosion resistance. All hinges to have an asymmetric end cap to ensure smooth location and weather tight sealing.
50. The release mechanism shall be an integral part of the hinge and shall self-relocate in one action on closure of the casement. All components, rivets and pins should withstand a force of 350N to comply with BS 6375 Part 2 2009, Specification for Operations and Strength Characteristics Loading of Windows Section A7 Test 6.0 and BS 8213 Part 1: 2004 - Design for Safety in Use and During Cleaning of Windows.              
51. Side hung windows must be restricted in compliance with BS 6375 Part 2 2009 Section A7 test 6.0. (Strength of Restricted Openings and Location Devices and Maximum Opening Stops). 
52. All habitable first floor rooms to have egress hinges, non-locking handles and child safety catches which must be fitted with a child-resistant release mechanism.
53. Components such as handles and locking mechanisms to be capable of offering adaptations (by mechanical or electrical means) in accordance with the Disability Discrimination Act Part 3 2005 and the housing providers Disability Equality Duty 2006.
54. Handle to be manufactured to BS EN ISO 9001 from die cast zinc alloy under with a polyester powder coating finish incorporating thermoplastic push fit covers. All components should be capable of sustaining a minimum of 30,000 cycles of operation without demonstrating any significant deterioration or deformation that would inhibit its function.
55. Handles to have option to provide non-latching facility to meet the considerations of the Disability Discrimination Act Part 3 2005 and the housing providers Disability Equality Duty 2006. Where non latching handles are fitted the window should also have attached the appropriate information warning label.  Locking mechanism must have option to offset handle height on side-hung sashes to meet the consideration of the Disability Discrimination Act Part 3 2005 and the housing providers Disability Equality Duty 2006. 
Hardware – Patio & French doors 
56. Door must come with all hardware necessary to properly function.
57. All external components must conform with requirements of BS EN 1670 2007 Class 4 corrosion resistance when tested in accordance with BSEN ISO 9227 2006. 
58. Cylinder
a. Euro profile
b. Double cylinder 
59. Locking mechanism to comply with BSEN 1303 2005 to the following minimum grades:
c. Durability to Grade 5
d. Key related security to Grade 4
e. Anti-pick and attack resistance to Grade 1
60. Compliant with SBD including meeting BS 3621 2007 “Thief resistant lock assembly – key egress” and PAS 24: 2012 section 8.5 cylinders for locks and Annex C (anti-manipulation)
Ventilation
61. Each window/door unit is to be fitted with colour-matched trickle ventilators, to meet Building Regulations (Part F1, 2010 plus relevant 2013 amendments). Ventilator to be secure and adjustable, complete with insect screen.  Ventilator to be through-frame type.
62. Where necessary, a frame extension profile, or extended leg framing, are to be used to ensure that trickle ventilators are clear of internal finishes. Frame extension sections to be of an identical material and finish to framing and designed to locate in grooves within the frame extrusion.
63. Where the window is of insufficient width to accommodate the level of ventilation required by Approved Document F1 the Contractor shall bring this to the attention of the Contract Administrator.
Window/Door Performance
64. Performance shall be as specified below to BS 6375, Part 1, 1989 and will achieve a Class A for mechanical testing to BS6375, Part 2.
a. Water Tightness……………………………………300 Pascals
b. Air Permeability…………………………………….600 Pascals
c. Wind Resistance
i. Casement …………………………………1600 Pascals
ii. Top hung & top swing fully reversible…..1200 Pascals
iii. Vertical sliding sash………………………1200 Pascals
iv. Door………………………………………	1200 Pascals
65. In certain coastal situations wind resistance of up to 2400 Pascals may be required. (any additional cost to be agreed with the client prior to order)
66. All framing including mullions, transoms and couplers shall be capable of withstanding the design wind loadings calculated in accordance with BS6399 Pt2: 1995
67. For new build windows are to be double glazed to achieve a U-value of 1.4 W/m2K or lower. Specific projects may require a lower U-value. Triple glazing may be specified where U-values of 0.8 W/m2K are required.
68. For new build maximum solar factor (‘g’ factor) on ground floor flat and bungalow windows shall be 0.39 W/m2K.  
69. For new build Patio/French doors are to achieve a U-value of 1.4 W/m2K or lower.
70. All horizontal lower rails of frames, transoms and sashes within a window shall be drained to allow water to escape.  
Surveys and Design
71. Every surveying and installation operative entering a tenant’s home shall have been DBS checked. 
72. The Contractor shall undertake surveys to take the dimensions and adjacent structural details of every window that is to be replaced.   
73. The surveys are to comply with BS 8213-4: 2007 “Windows, doors and rooflights – Part 4: Code of practice for the survey and installation of windows and external doorsets” 
74. For new build the manufacturer will be required to liaise with the builder and/or frame manufacturer on window sizes.
75. The Contractor will arrange survey appointments with tenants.
76. Should the Contractor be unable to gain access on the first visit he will make one additional appointment. If on the second appointment he is unable to gain access then he will inform the Client.
77. A drawing or photograph of the existing window configuration will be provided for each property surveyed.
78. A costed property window schedule and drawing of the replacement window configuration to be provided to the client prior to fabrication.
79. Unless agreed otherwise with the client, maximum lead time from notification of requirement to survey being undertaken will be 4 weeks.
80. Maximum lead time from survey to installation unless agreed otherwise with the client will be 8 weeks 
81. Where the installation is for Flats requiring planning permission, we require the supplier to submit the planning application with reimbursement of fee and other costs on application. Copies of documentation to be provided to the Client. 
82. Where the survey identifies that there is through window venting for an open flue gas appliance within the room then the Contractor will inform the client to ascertain whether another through window vent is to be installed or whether the Client will engage others to provide a through wall solution.
Installation 
83. Every surveying and installation operative entering a tenant’s home shall have been DBS checked. 
84. Every surveying and installation operative shall have a valid accredited asbestos awareness certificate 
85. The Contractor is responsible for ensuring that all new windows are square and central in the opening, and that a perimeter gap shall be provided to allow adequate thermal expansion and contraction of the framing, consistent with the site location and limitations of the perimeter sealant used.   
86. Window framing to be securely fixed direct to the building structure, between 150mm and 200mm from each corner and at centers not exceeding 600mm, as laid down in procedures issued by the systems company.    
87. All installation shall be in accordance with BS8213 Part 4 2016.  
88. The removal of existing windows and doors must be programmed to ensure that units are only removed if they are to be replaced within the same working day.   
89. At the end of each day, the removed windows and doors, together with any debris associated with the removal of the removed units, are to be cleared away and subsequently disposed of at an approved recycling facility. 
90. No removed items to be left with the tenant. 
91. At the end of each day, the Contractor shall be responsible for the removal of any debris from the new materials from site and shall thoroughly clean the working area.
92. On removal of the existing windows, doors and associated frames, sub frames, cills etc. the reveal surfaces of the opening are to be cleaned to remove all existing frame sealant, mastic, beading mortar etc. ready for the installation of the new units.
93. Where DPC materials require repair or renewal the Client must be informed. The Contractor is to make all due allowance to ensure that no damage is caused to the property internally or externally.   The Contractor’s attention is drawn specifically to the need to protect soft landscaping and external and internal fabric and finishes. Any damage caused as a result of the replacement of windows and doors will be the Contractor’s liability.
94. The Contractor shall allow for all necessary making good of all work disturbed including external decoration.
95. As part of the window removal process the installer must ensure that insulation does not escape from cavities and should address this in method statements.
96. Frames are to be positioned to cover the cavity within the reveals, and level with the existing external window line wherever possible, ensuring that they are plumb, level and without bow.
97. Any gap between the internal frame face and the existing wall structure line is to be filled with expanding foam void filler, knifed off flush with the wall structure. The foam and a minimum of 15mm of plaster is to be covered with PVCu trims from a product range which carries BBA certification or Kite marking to BS 7619: 1993. Trims to be fixed with acrylic caulking.
98. Existing sliding sash boxes and all associated trims are to be removed.   In the case of rebated reveals the Contractor is to make up the rebate dimension internally with treated softwood or PVCu, such that the reveal is made flush. Internal PVCu linings are to be applied to the satisfaction of the Client. No timber shall be exposed to moisture and the Contractor shall provide a detail drawing showing his solution for the Client’s approval prior to manufacture.
99. Where integral timber cills and sub frames with any existing windows are removed new PVCu cills to be provided and fitted. Should any glazing be broken on removal, all glass must be immediately cleaned up, both internally and externally. 
100. The Contractor is to allow for necessary measures to protect the occupants, fittings and finishes within the rooms for the duration of the works.
101. For refurbishment work seal all external joints between framing and structure with low modulus neutral cure silicone sealant to BS5889 (1989).  Sealants shall be tested and classified in accordance with BS EN ISO 11600 and of low modulus and high elasticity, with movement capability of at least 20%, class 20LM or 25LM (Sealing on New Build project is not included unless this is carried out at the same time as the installation). Silicone colour to match the frame. 
102. Unclipping all existing telephone cables, aerial cables and the like from existing windows and door frames, and re-clip to surround in a suitable location using new cable clips of appropriate size and colour. Any cables passing through a frame/structure joint shall be routed through a plastic sleeve, the inner end of which is to be higher than the outer to prevent water penetration along or through the sleeve (for the avoidance of doubt the supplier is not to reposition satellite dishes. Where it is identified at survey stage that this is an issue the Client must be informed)
103. Remove and re-fit existing net curtains and other soft furnishings as applicable. Curtain rods to be screw fixed to window frame head. Contractor to replace curtain rods where existing are damaged during installation. 
104. The Contractor will provide programme information in advance
105. All packaging must be recyclable.  
106. Installation of fenestration systems shall be performed in accordance with drawings.  
107. After installation and glazing the Contractor shall check and adjust, if required, all items furnished.
108. The contractor is to provide the resident with a simple maintenance handbook.
109. Rectification of installation and product issues – 24 hours for security and H&S issues; within 10 working days for other issues.
Preliminaries
1. NHF Preliminaries as provided with the ITT
2. Please note that the following clauses within the Preliminaries only apply to contracts from the framework if detailed by the Member: 
2.1. Clause 2.2
2.2. Clause 2.3
2.3. Clause 2.4
2.4. Clause 3.4
2.5. Clause 6.2
2.6. Clause 6.4
2.7. Clause 7.2
2.8. Clause 10 except 10.3.6 and 10.3.7 which are included
2.9. Clause 11
2.10. Clause 12
2.11. Clause 13



Warranty
1. Installations are to be registered with FENSA within 14 days of installation.
2. Warranties:
· 10 years on frame including sashes and external cills
· 10 years on glazing
· 10 years on hardware
3. Warranties to be parent company (where available) backed for a minimum of 10 years
4. Insurance backed warranties to be available.
5. Training to maintenance teams (in-house and contractor) free of charge
6. Spare parts, “first aid kits” available Free of charge during warranty period. First aid kits to include as a minimum: handles, hinges, locks, vents, gearbox, gasket 
7. Availability of parts outside of warranty, to exceed the life of the framework 

NON-Warranty PARTS REPLACEMENT
Any orders for parts not covered by the warranty i.e. fair wear and tear or damaged due to misuse, should be sent through to Sharon.Durrance@wrekin-windows.co.uk  along with any photos and detail on lengths of hinges, locking mechanisms or trickle vents required.
Performance Requirements

Contract performance monitoring will be monitored using the following methods and reported 6-monthly:

Inspection measurement KPIs
These to be measured at Member level

Product Quality	agreed warranty claims not to exceed 2% of windows & patio doors installed.

Delivery 	windows delivered complete, on time and undamaged not to be less than 98%. 

Installation 	windows installed complete, on time and undamaged not to be less than 98%. 

Speed of defects 	product/installation defect issues that go over 28 days not to exceed
        resolution	2% of windows and patio doors installed. Where security or weather tightness are compromised the repair must be completed within 24 hours of report.

Speed of warranty	warranty issues that go over 28 days not to exceed 2% of windows
        resolution 	and patio doors installed. Where security or weather tightness are compromised the repair must be completed within 24 hours of report.

Default notices
These to be applied at Member level 
Product Quality 	where warranty claims exceed 2% of the product purchased £25 for each claim in excess of the 2% percentage.

Delivery accuracy	where the number of windows & patio doors delivered complete, on time and undamaged is less than 98%, £25 for each window below the 98% percentage 

Installation	where the number of windows & patio doors installed complete, on time, undamaged and correctly first time is less than 98% of windows installed, £25 for each window below the 98% percentage.

Speed of Defects 	product/installation defect issues that go over 28 days exceed 2% of windows
      resolution 	& patio doors installed, £25 for each window above 2%.  

In addition, where security or weather tightness issues are not repaired within 24 hours of report the client reserves the right to instigate the repair with a third party and recharge the supplier plus a £25 admin charge.

Speed of warranty	where warranty issues that go over 28 days exceed 2% of windows & patio 
resolution 	doors installed, £25 for each window above 2%. 

In addition, where security or weather tightness issues are not repaired within 24 hours of report the client reserves the right to instigate the repair with a third party and recharge the supplier plus a £25 admin charge.


window designs
Wrekin Style 20					Wrekin Style 74	
[image: UH017]					[image: UH036]


		Wrekin Style 131				Wrekin Style 1
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		Wrekin Style 127				Wrekin Style 40
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pricing (supply only) Double glazing

	 
	Style 74: Clear laminated glass, Ground Floor 

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	501-650
	£186.03
	£189.44
	£192.85
	£197.99
	£207.32
	£216.48
	£224.57

	
	651-800
	£187.74
	£192.85
	£196.28
	£201.40
	£210.77
	£225.28
	£235.26

	
	801-950
	£194.55
	£199.69
	£206.51
	£213.33
	£224.60
	£242.89
	£256.65

	
	951-1100
	£199.69
	£206.51
	£216.75
	£228.70
	£243.61
	£262.23
	£281.61

	
	1101-1250
	£206.51
	£212.10
	£224.55
	£244.04
	£260.87
	£283.36
	£304.78

	
	1251-1400
	£216.75
	£232.12
	£245.79
	£261.12
	£278.16
	£302.74
	£326.17

	
	1401-1550
	£240.14
	£245.32
	£259.15
	£270.17
	£295.43
	£329.73
	£342.21

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	 
	Style 74: Obscured laminated glass, Ground Floor

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	501-650
	£205.93
	£209.45
	£214.73
	£220.01
	£227.05
	£239.37
	£256.97

	
	651-800
	£209.45
	£212.97
	£218.24
	£223.54
	£230.57
	£242.89
	£260.49

	
	801-950
	£216.48
	£220.01
	£228.80
	£237.60
	£246.40
	£264.00
	£285.13

	
	951-1100
	£221.76
	£228.80
	£241.13
	£255.21
	£269.29
	£285.13
	£302.74

	
	1101-1250
	£228.80
	£244.64
	£258.73
	£274.56
	£290.41
	£313.29
	£329.12

	
	1251-1400
	£241.13
	£258.73
	£278.07
	£295.69
	£313.29
	£332.64
	£350.25

	
	1401-1550
	£264.00
	£279.84
	£299.20
	£316.80
	£337.93
	£357.29
	£374.89

	
	
	
	
	
	
	
	
	

	 
	Style 74: Clear standard glass, Ground Floor 

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	501-650
	£158.72
	£160.42
	£163.84
	£168.98
	£177.95
	£191.85
	£203.19

	
	651-800
	£160.42
	£163.84
	£168.98
	£174.10
	£186.58
	£197.13
	£208.52

	
	801-950
	£167.26
	£172.36
	£179.21
	£184.32
	£200.40
	£211.20
	£224.57

	
	951-1100
	£172.36
	£180.91
	£189.44
	£196.28
	£212.50
	£225.28
	£242.40

	
	1101-1250
	£180.91
	£183.62
	£192.56
	£208.21
	£224.60
	£239.37
	£256.65

	
	1251-1400
	£191.77
	£202.15
	£212.50
	£222.87
	£236.69
	£253.43
	£267.33

	
	1401-1550
	£207.68
	£218.24
	£224.42
	£225.92
	£255.21
	£265.76
	£283.39

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	 
	Style 74: Obscured standard glass, Ground Floor

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	501-650
	£164.69
	£167.97
	£174.95
	£186.03
	£189.44
	£196.28
	£204.81

	
	651-800
	£169.97
	£174.95
	£178.30
	£191.16
	£197.99
	£204.81
	£213.33

	
	801-950
	£180.91
	£186.03
	£192.85
	£203.09
	£211.62
	£220.16
	£232.12

	
	951-1100
	£187.74
	£194.55
	£204.81
	£216.75
	£226.98
	£235.52
	£247.49

	
	1101-1250
	£194.55
	£206.51
	£216.75
	£230.41
	£240.65
	£250.89
	£267.95

	
	1251-1400
	£204.81
	£216.75
	£228.70
	£242.35
	£254.31
	£267.95
	£286.73

	
	1401-1550
	£216.75
	£221.88
	£242.35
	£256.01
	£267.95
	£286.73
	£307.21

	
	
	
	
	
	
	
	
	

	 
	Style 74: Clear glass, First Floor

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	501-650
	£163.84
	£167.26
	£170.67
	£175.79
	£181.39
	£193.61
	£206.76

	
	651-800
	£167.26
	£170.67
	£175.79
	£184.32
	£191.77
	£202.41
	£213.88

	
	801-950
	£177.49
	£180.91
	£186.03
	£194.55
	£205.58
	£218.24
	£231.70

	
	951-1100
	£184.32
	£187.74
	£196.28
	£206.51
	£219.41
	£232.32
	£244.19

	
	1101-1250
	£192.85
	£196.28
	£199.79
	£208.59
	£231.50
	£244.64
	£260.22

	
	1251-1400
	£203.87
	£209.05
	£216.75
	£228.70
	£243.61
	£258.73
	£276.26

	
	1401-1550
	£215.95
	£221.14
	£233.23
	£245.32
	£257.43
	£278.04
	£292.30

	
	
	
	
	
	
	
	
	

	 
	Style 74: Obscured glass, First Floor

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	501-650
	£165.43
	£169.90
	£179.21
	£188.31
	£191.77
	£202.41
	£211.20

	
	651-800
	£174.10
	£179.21
	£182.63
	£193.49
	£200.40
	£211.20
	£220.01

	
	801-950
	£180.91
	£186.03
	£192.85
	£205.58
	£214.23
	£227.05
	£239.37

	
	951-1100
	£187.74
	£194.55
	£204.81
	£219.41
	£229.78
	£242.89
	£255.21

	
	1101-1250
	£194.55
	£206.51
	£216.75
	£233.23
	£243.61
	£258.73
	£276.33

	
	1251-1400
	£207.32
	£219.41
	£231.50
	£245.32
	£257.43
	£276.33
	£295.69

	
	1401-1550
	£219.41
	£224.60
	£245.32
	£264.00
	£276.33
	£295.69
	£316.80



	
	
	Style No: 131 Clear laminated glass, Ground Floor

	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150
	2151-2300

	801-950
	£279.94
	£284.92
	£289.89
	£303.13
	£311.43

	951-1100
	£296.51
	£303.13
	£314.74
	£327.99
	£339.58

	1101-1250
	£313.07
	£324.85
	£337.93
	£352.84
	£366.08

	1251-1400
	£334.61
	£346.19
	£359.46
	£377.69
	£390.94

	1401-1550
	£361.12
	£366.08
	£384.31
	£390.37
	£405.02

	 
	 
	 
	 
	 
	 

	Style No: 131 Obscured laminated glass, Ground Floor

	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150
	2151-2300

	801-950
	£300.96
	£306.26
	£313.29
	£325.60
	£336.16

	951-1100
	£320.32
	£327.37
	£339.69
	£355.53
	£366.08

	1101-1250
	£339.69
	£352.01
	£364.32
	£381.94
	£396.01

	1251-1400
	£360.83
	£374.89
	£388.98
	£408.32
	£424.18

	1401-1550
	£351.38
	£367.50
	£380.39
	£401.34
	£422.30

	 
	 
	 
	 
	 
	 

	Style No: 131 Clear standard glass, Ground Floor

	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150
	2151-2300

	801-950
	£245.17
	£248.48
	£255.11
	£266.69
	£274.98

	951-1100
	£258.43
	£265.05
	£273.33
	£284.92
	£294.85

	1101-1250
	£273.33
	£280.59
	£289.89
	£303.13
	£313.07

	1251-1400
	£286.58
	£296.51
	£306.45
	£319.70
	£329.64

	1401-1550
	£303.13
	£314.74
	£324.68
	£329.76
	£340.56

	 
	 
	 
	 
	 
	 

	Style No: 131 Obscured standard glass, Ground Floor

	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150
	2151-2300

	801-950
	£280.73
	£286.01
	£293.05
	£305.37
	£314.17

	951-1100
	£296.58
	£305.37
	£315.94
	£328.26
	£338.81

	1101-1250
	£314.17
	£324.75
	£335.29
	£349.38
	£361.69

	1251-1400
	£331.78
	£344.10
	£354.65
	£370.50
	£382.81

	1401-1550
	£354.65
	£366.98
	£375.78
	£395.14
	£407.47

	 
	 
	 
	 
	 
	 

	Style No: 131 Clear glass, First Floor

	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150
	2151-2300

	801-950
	£267.95
	£271.37
	£278.20
	£290.14
	£298.66

	951-1100
	£281.61
	£288.44
	£296.96
	£308.91
	£319.16

	1101-1250
	£296.96
	£296.28
	£314.03
	£317.99
	£337.93

	1251-1400
	£302.28
	£320.86
	£331.11
	£344.76
	£348.26

	1401-1550
	£324.26
	£334.52
	£341.33
	£345.45
	£356.25

	 
	 
	 
	 
	 
	 

	Style No: 131 Obscured glass, First Floor

	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150
	2151-2300

	801-950
	£286.89
	£292.17
	£299.20
	£311.52
	£320.32

	951-1100
	£302.74
	£311.52
	£322.09
	£334.42
	£344.96


[image: ]
		
	Style 1: Clear laminated glass, Ground Floor

	Width
	351-500
	501-650
	651-800
	801-950
	951-1100
	1101-1250
	1251-1400

	351-500
	£45.76
	£47.53
	£49.27
	£52.79
	£58.09
	£65.11
	£72.16

	501-650
	£47.53
	£49.27
	£54.57
	£63.36
	£70.39
	£77.44
	£87.99

	651-800
	£52.79
	£54.57
	£63.36
	£73.92
	£82.72
	£73.92
	£102.09

	801-950
	£59.84
	£61.60
	£72.16
	£82.72
	£93.29
	£105.62
	£117.92

	951-1100
	£65.11
	£68.65
	£80.96
	£93.29
	£105.62
	£117.92
	£132.00

	1101-1250
	£72.16
	£75.68
	£89.77
	£97.43
	£117.92
	£132.00
	£147.86

	1251-1400
	£79.20
	£82.72
	£98.55
	£114.41
	£128.48
	£144.32
	£161.92

	 
	 
	 
	 
	 
	
	 
	 

	Style 1: Obscured laminated glass, Ground Floor
	 
	 
	 

	Width
	351-500
	501-650
	651-800
	801-950
	951-1100
	1101-1250
	1251-1400

	351-500
	£51.04
	£52.79
	£54.57
	£58.09
	£65.11
	£72.16
	£80.96

	501-650
	£52.79
	£54.57
	£61.60
	£70.39
	£79.20
	£87.99
	£98.55

	651-800
	£55.45
	£57.45
	£72.16
	£82.72
	£93.29
	£105.62
	£117.92

	801-950
	£65.11
	£70.39
	£82.72
	£95.05
	£109.13
	£121.45
	£135.52

	951-1100
	£72.16
	£73.47
	£93.29
	£107.35
	£123.21
	£137.29
	£154.88

	1101-1250
	£80.09
	£81.47
	£103.84
	£119.68
	£137.29
	£153.11
	£172.49

	1251-1400
	£87.99
	£89.46
	£114.41
	£132.00
	£151.37
	£170.71
	£191.85

	 
	 
	 
	 
	 
	
	 
	 

	Style 1: Clear standard glass, Ground Floor
	 
	 
	 
	 

	Width
	351-500
	501-650
	651-800
	801-950
	951-1100
	1101-1250
	1251-1400

	351-500
	£36.96
	£38.73
	£40.48
	£43.99
	£49.27
	£54.57
	£59.84

	501-650
	£38.73
	£40.48
	£45.76
	£51.04
	£56.32
	£61.60
	£68.65

	651-800
	£42.24
	£43.99
	£51.04
	£58.09
	£63.36
	£70.39
	£79.20

	801-950
	£47.53
	£49.27
	£56.32
	£63.36
	£72.16
	£79.20
	£87.99

	951-1100
	£51.04
	£54.57
	£61.60
	£70.39
	£79.20
	£86.24
	£96.80

	1101-1250
	£54.57
	£58.09
	£68.65
	£72.45
	£86.24
	£95.05
	£105.62

	1251-1400
	£59.84
	£63.36
	£73.92
	£82.72
	£93.29
	£103.84
	£116.16

	 
	 
	 
	 
	 
	
	 
	 

	Style 1: Obscured standard glass, Ground Floor
	 
	 
	 

	Width
	351-500
	501-650
	651-800
	801-950
	951-1100
	1101-1250
	1251-1400

	351-500
	£38.73
	£40.48
	£42.24
	£47.53
	£52.79
	£58.09
	£65.11

	501-650
	£40.48
	£42.24
	£49.27
	£54.57
	£61.60
	£68.65
	£75.68

	651-800
	£43.99
	£45.43
	£56.32
	£63.36
	£70.39
	£77.44
	£87.99

	801-950
	£52.79
	£54.57
	£61.60
	£70.39
	£79.20
	£87.99
	£98.55

	951-1100
	£56.32
	£55.86
	£68.65
	£79.20
	£87.99
	£98.55
	£109.13

	1101-1250
	£60.72
	£61.04
	£75.68
	£86.24
	£96.80
	£107.35
	£121.45

	1251-1400
	£65.11
	£66.24
	£82.72
	£95.05
	£105.62
	£117.92
	£132.00

	
	
	
	
	
	
	
	

	Style 1: Clear glass, First Floor

	Width
	351-500
	501-650
	651-800
	801-950
	951-1100
	1101-1250
	1251-1400

	351-500
	£36.96
	£38.73
	£40.48
	£43.99
	£49.27
	£54.57
	£59.84

	501-650
	£38.73
	£40.48
	£45.76
	£51.04
	£56.32
	£61.60
	£68.65

	651-800
	£42.24
	£43.99
	£51.04
	£58.09
	£63.36
	£70.39
	£79.20

	801-950
	£47.53
	£49.27
	£56.32
	£63.36
	£72.16
	£79.20
	£87.99

	951-1100
	£51.04
	£54.57
	£61.60
	£70.39
	£79.20
	£86.24
	£96.80

	1101-1250
	£54.57
	£58.09
	£68.65
	£72.45
	£86.24
	£95.05
	£105.62

	1251-1400
	£59.84
	£63.36
	£73.92
	£82.72
	£93.29
	£103.84
	£116.16

	
	
	
	
	
	
	
	

	Style 1: Obscured Glass, First Floor

	Width
	351-500
	501-650
	651-800
	801-950
	951-1100
	1101-1250
	1251-1400

	351-500
	£38.73
	£40.48
	£42.24
	£47.53
	£52.79
	£58.09
	£65.11

	501-650
	£40.48
	£42.24
	£49.27
	£54.57
	£61.60
	£68.65
	£75.68

	651-800
	£43.99
	£45.45
	£56.32
	£63.36
	£70.39
	£77.44
	£87.99

	801-950
	£52.79
	£54.57
	£61.60
	£70.39
	£79.20
	£87.99
	£98.55

	951-1100
	£56.32
	£55.86
	£68.65
	£79.20
	£87.99
	£98.55
	£109.13

	1101-1250
	£60.72
	£61.04
	£75.68
	£86.24
	£96.80
	£107.35
	£121.45

	1251-1400
	£65.11
	£66.24
	£82.72
	£95.05
	£105.62
	£117.92
	£132.00

	
	
	
	
	
	
	
	



V170401


	 
	Style 127: Clear laminated glass, Ground Floor

	 
	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150

	Height
	651-800
	£205.73
	£212.46
	£230.57
	£247.30

	
	801-950
	£224.26
	£234.38
	£255.21
	£272.57

	
	951-1100
	£246.19
	£253.17
	£281.61
	£301.47

	
	1101-1250
	£266.42
	£274.84
	£306.26
	£328.54

	
	1251-1400
	£286.66
	£296.34
	£330.89
	£355.59

	
	1401-1550
	£319.39
	£343.21
	£366.46
	£384.50

	
	
	
	
	
	

	 
	Style 127: Obscured laminated glass, Ground Floor

	 
	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150

	Height
	651-800
	£234.67
	£245.51
	£256.32
	£267.17

	
	801-950
	£258.14
	£270.78
	£285.21
	£297.85

	
	951-1100
	£285.21
	£299.65
	£315.92
	£330.35

	
	1101-1250
	£310.49
	£328.54
	£344.80
	£362.83

	
	1251-1400
	£335.76
	£355.59
	£375.49
	£393.54

	
	1401-1550
	£362.83
	£382.68
	£407.95
	£427.83

	
	
	
	
	
	

	 
	Style 127: Clear standard glass, Ground Floor

	 
	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150

	Height
	651-800
	£186.56
	£191.85
	£198.88
	£211.20

	
	801-950
	£202.61
	£209.48
	£221.76
	£234.67

	
	951-1100
	£214.17
	£218.15
	£241.13
	£254.53

	
	1101-1250
	£229.33
	£233.99
	£258.73
	£274.38

	
	1251-1400
	£244.51
	£249.50
	£276.33
	£292.44

	
	1401-1550
	£267.86
	£278.17
	£305.08
	£312.28

	
	
	
	
	
	

	 
	Style 127: Obscured standard glass, Ground Floor

	 
	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150

	Height
	651-800
	£198.56
	£205.79
	£214.82
	£222.03

	
	801-950
	£222.03
	£231.07
	£240.08
	£249.11

	
	951-1100
	£241.88
	£252.73
	£261.75
	£272.57

	
	1101-1250
	£259.95
	£270.78
	£281.61
	£294.23

	
	1251-1400
	£278.00
	£290.63
	£303.27
	£315.92

	
	1401-1550
	£299.65
	£312.28
	£324.93
	£337.57

	
	
	
	
	
	

	 
	Style 127: Clear glass, First Floor

	 
	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150

	Height
	651-800
	£204.17
	£209.45
	£216.48
	£229.26

	
	801-950
	£219.79
	£232.32
	£239.37
	£252.73

	
	951-1100
	£231.02
	£235.19
	£258.73
	£272.57

	
	1101-1250
	£246.19
	£251.01
	£276.33
	£292.44

	
	1251-1400
	£261.38
	£266.53
	£293.93
	£310.49

	
	1401-1550
	£285.04
	£293.64
	£323.13
	£333.95

	
	
	
	
	
	

	 
	Style 127: Obscured glass, First Floor

	 
	Width
	1551-1700
	1701-1850
	1851-2000
	2001-2150

	Height
	651-800
	£216.63
	£223.84
	£232.85
	£240.08

	
	801-950
	£240.08
	£249.11
	£258.14
	£267.17

	
	951-1100
	£259.95
	£270.78
	£279.81
	£290.63

	
	1101-1250
	£278.00
	£288.84
	£301.47
	£312.28

	
	1251-1400
	£296.05
	£308.68
	£321.31
	£333.95

	
	1401-1550
	£315.92
	£330.35
	£342.98
	£359.23



	 
	Style 40: Clear laminated glass Ground Floor 

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	651-800
	£123.63
	£127.05
	£137.29
	£146.08
	£154.88
	£163.69
	£174.23

	
	801-950
	£133.93
	£137.35
	£151.37
	£161.92
	£174.23
	£184.80
	£195.35

	
	951-1100
	£142.52
	£151.12
	£157.57
	£179.52
	£191.85
	£204.17
	£216.48

	
	1101-1250
	£152.82
	£164.83
	£171.79
	£197.13
	£211.20
	£223.54
	£237.60

	
	1251-1400
	£163.12
	£178.59
	£185.78
	£212.97
	£228.80
	£244.64
	£258.73

	
	1401-1550
	£179.52
	£200.64
	£214.73
	£230.57
	£249.92
	£265.76
	£281.61

	
	
	
	
	
	
	
	
	

	 
	Style 40: Obscured laminated glass, Ground Floor

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	651-800
	£140.81
	£142.61
	£151.63
	£164.27
	£175.11
	£185.93
	£196.75

	
	801-950
	£151.63
	£157.04
	£169.67
	£182.34
	£196.75
	£209.40
	£222.03

	
	951-1100
	£162.46
	£173.30
	£189.57
	£203.98
	£218.43
	£234.67
	£249.11

	
	1101-1250
	£173.30
	£189.57
	£207.59
	£223.84
	£241.88
	£258.14
	£276.18

	
	1251-1400
	£185.93
	£205.79
	£225.65
	£243.70
	£263.56
	£283.40
	£301.47

	
	1401-1550
	£0.00
	£0.00
	£0.00
	£0.00
	£0.00
	£0.00
	£0.00

	
	
	
	
	
	
	
	
	

	 
	Style 40: Clear standard glass Ground Floor 

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	651-800
	£104.75
	£108.17
	£117.92
	£123.21
	£130.25
	£135.52
	£142.56

	
	801-950
	£115.05
	£120.21
	£130.25
	£137.29
	£144.32
	£153.11
	£160.17

	
	951-1100
	£123.63
	£130.51
	£133.14
	£149.60
	£158.40
	£167.20
	£174.23

	
	1101-1250
	£130.51
	£139.09
	£143.27
	£161.92
	£170.71
	£179.52
	£188.34

	
	1251-1400
	£142.56
	£153.11
	£153.23
	£172.49
	£183.04
	£193.61
	£202.41

	
	1401-1550
	£153.11
	£167.20
	£177.76
	£184.80
	£198.88
	£211.20
	£220.01

	
	
	
	
	
	
	
	
	

	 
	Style 40: Obscured standard glass, Ground Floor

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	651-800
	£115.54
	£119.15
	£126.35
	£133.57
	£140.81
	£149.83
	£157.04

	
	801-950
	£126.35
	£133.57
	£140.81
	£149.83
	£158.86
	£167.89
	£176.90

	
	951-1100
	£135.38
	£144.41
	£155.24
	£164.27
	£175.11
	£184.13
	£194.95

	
	1101-1250
	£144.41
	£157.04
	£167.89
	£178.71
	£189.57
	£200.37
	£211.20

	
	1251-1400
	£155.24
	£167.89
	£180.54
	£191.35
	£203.98
	£216.63
	£229.26

	
	1401-1550
	£169.67
	£184.13
	£196.75
	£207.59
	£222.03
	£236.48
	£252.73

	
	
	
	
	
	
	
	
	

	 
	Style 40: Clear glass, First Floor

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	651-800
	£113.34
	£116.75
	£126.73
	£132.00
	£139.04
	£144.32
	£151.37

	
	801-950
	£123.63
	£128.77
	£139.04
	£146.08
	£153.11
	£161.92
	£168.98

	
	951-1100
	£132.21
	£139.09
	£141.69
	£158.40
	£167.20
	£176.01
	£183.04

	
	1101-1250
	£139.09
	£147.68
	£151.79
	£170.71
	£179.52
	£188.34
	£197.13

	
	1251-1400
	£147.68
	£157.99
	£161.76
	£181.28
	£191.85
	£202.41
	£211.20

	
	1401-1550
	£161.92
	£174.23
	£186.56
	£195.35
	£209.45
	£220.01
	£228.80

	
	
	
	
	
	
	
	
	

	 
	Style 40: Obscured glass, First Floor

	 
	Width
	801-950
	951-1100
	1101-1250
	1251-1400
	1401-1550
	1551-1700
	1701-1850

	Height
	651-800
	£124.55
	£128.18
	£135.38
	£142.61
	£151.63
	£158.86
	£166.08

	
	801-950
	£135.38
	£142.61
	£149.83
	£158.86
	£167.89
	£176.90
	£185.93

	
	951-1100
	£144.41
	£153.44
	£164.27
	£173.30
	£184.13
	£193.16
	£203.98

	
	1101-1250
	£155.24
	£166.08
	£176.90
	£187.74
	£198.56
	£209.40
	£220.22

	
	1251-1400
	£164.27
	£176.90
	£189.57
	£200.37
	£213.00
	£225.65
	£238.28

	
	1401-1550
	£176.90
	£191.35
	£205.79
	£214.82
	£231.07
	£245.51
	£259.95












pricing (ADDITIONAL ITEMS)

	Patio Doors
	 
	 

	French doors 2000-2200 (h) x 1700-1900 (w) retrofit
	£609.76
	each

	French doors 2000-2200 (h) x 1700-1900 (w) new build
	£609.76
	each

	Sliding doors 2000-2200 (h) x 1700-1900 (w)
	£735.60
	each

	
	
	

	
	
	

	Installation
	
	 

	Retrofit Window
	£97.20
	each

	New Build Window
	£59.05
	each

	 
	 
	 

	Retrofit French / Patio Door
	£160.76
	each

	New Build French / Patio Door
	£122.75
	each

	 
	 
	 

	Remove and make good sliding sash
	£160.76
	each
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Width 351-500 501-650 651-800 801-950 951-11001101-1250

351-500

£116.05 £117.77 £122.87 £127.99 £129.71 £136.53

501-650

£117.77 £119.48 £124.59 £129.71 £131.42 £138.24

651-800

£119.48 £121.18 £126.30 £131.42 £136.53 £139.94

801-950

£122.87 £124.59 £129.71 £133.13 £143.37 £153.60

951-1100

£126.30 £127.99 £133.13 £143.37 £155.32 £165.55

1101-1250

£129.71 £131.42 £138.24 £148.80 £165.55 £179.21

1251-1400

£133.13 £134.83 £145.08 £158.38 £177.49 £192.85

Width 351-500 501-650 651-800 801-950 951-11001101-1250

351-500

£117.77 £122.87 £115.19 £134.83 £139.94 £150.20

501-650

£118.60 £123.74 £120.13 £136.53 £141.66 £148.48

651-800

£119.48 £124.59 £127.99 £138.24 £143.37 £150.20

801-950

£120.32 £126.30 £131.42 £145.08 £155.32 £167.26

951-1100

£121.18 £129.71 £141.66 £157.02 £170.67 £182.63

1101-1250

£122.87 £136.53 £151.90 £168.98 £184.32 £197.99

1251-1400

£129.71 £145.08 £162.13 £180.91 £197.99 £215.05

Width 351-500 501-650 651-800 801-950 951-11001101-1250

351-500

£90.44 £92.14 £97.29 £105.81 £112.65 £119.48

501-650

£92.14 £93.89 £98.99 £107.52 £114.34 £121.18

651-800

£93.89 £95.58 £100.70 £109.22 £116.05 £122.87

801-950

£95.58 £97.29 £104.11 £114.34 £122.87 £131.42

951-1100

£98.99 £100.70 £109.22 £121.18 £129.71 £138.24

1101-1250

£104.11 £105.81 £114.34 £123.35 £136.53 £146.78

1251-1400

£105.81 £109.22 £119.48 £129.48 £145.08 £155.32

Width 351-500 501-650 651-800 801-950 951-11001101-1250

351-500

£117.77 £122.87 £124.59 £134.83 £139.94 £150.20

501-650

£118.60 £123.74 £126.30 £136.53 £141.66 £148.48

651-800

£119.48 £124.59 £127.99 £138.24 £143.37 £150.20

801-950

£120.32 £126.30 £131.42 £145.08 £155.32 £167.26

951-1100

£121.18 £129.71 £141.66 £157.02 £170.67 £182.63

1101-1250

£122.87 £136.53 £151.90 £168.98 £184.32 £197.99

1251-1400

£129.71 £145.08 £162.13 £180.91 £197.99 £215.05

Width 351-500 501-650 651-800 801-950 951-11001101-1250

351-500

£90.44 £92.14 £97.29 £105.81 £110.94 £117.77

501-650

£92.14 £93.89 £98.99 £107.52 £114.34 £119.48

651-800

£93.89 £95.58 £100.70 £109.22 £116.05 £122.87

801-950

£95.58 £97.29 £104.11 £114.34 £122.87 £131.42

951-1100

£98.99 £100.70 £109.22 £121.18 £129.71 £138.24

1101-1250

£102.41 £105.81 £114.34 £127.99 £136.53 £146.78

1251-1400

£105.81 £109.22 £119.48 £133.13 £145.08 £155.32

Width 351-500 501-650 651-800 801-950 951-11001101-1250

351-500

£117.77 £122.87 £124.59 £134.83 £139.94 £150.20

501-650

£118.60 £123.74 £126.30 £136.53 £141.66 £148.48

651-800

£119.48 £124.59 £127.99 £138.24 £143.37 £150.20

801-950

£120.32 £126.30 £131.42 £145.08 £155.32 £167.26

951-1100

£121.18 £129.71 £141.66 £157.02 £170.67 £182.63

1101-1250

£122.87 £136.53 £151.90 £168.98 £184.32 £197.99

1251-1400

£129.71 £145.08 £162.13 £180.91 £197.99 £215.05

Style 20: Clear laminated glass, Ground Floor

Height

Style 20: Obscured laminated glass, Ground Floor

Height

Style 20: Clear standard glass, Ground Floor

Style 20: Obscured glass, First Floor

Height

Height

Style 20: Obscured standard glass, Ground Floor

Height

Style 20: Clear glass, First Floor

Height
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